[Menu]>[Circuits Gallery]>[Light controller]

Parts explanation
of Light controller

PIC16F873 In this circuit, PIC16F873 is used. And compare feature and A/D converter feature are used. Data sheet for PIC16F873 3 terminal regulator ( 78L05 ) This regulator is used to make the stable power of +5V. The maximum output current is 100 mA. Data sheet for 78L05 Transistor for the MOS FET drive ( 2SC1815 ) This transistor is used to drive MOS FET by the output of PIC. It is converting the output of PIC (0V to 5V) into the voltage to control an FET (0V to 12V). Data sheet for 2SC1815 Power MOS FET ( 2SJ471 ) This is P channel MOS FET. The maximum drain current is 30A. When the FET is in the ON condition, the resistance between drain and source is 25 milli-ohm. So, the electric power loss when the 10-A electric current flows in the ON condition is 2.5 W. Data sheet for 2SJ471 Heat sink Because the ON resistance of 2SJ471 is 25 miliohms, the heat generation is not so big. The size of heat sink is the 25-mm height, the 23-mm width of the surface which installs the MOS FET and the 10-mm depth to the direction of fin. I think that it is too big a little. IC socket PIC16F873 is 28 pins of the slim type. When you can not get a slim-type 28 pin socket, two sockets of 14 pins can be used. In this circuit, I used two 14 pin sockets. Resonator I used 10-MHz resonator. When changing the frequency of resonator, the value with all kinds on the software must be changed. Variable resistor for the voltage control I used B type. Resistor I used 1/8W as all resistors. Multilayer ceramic capacitor These capacitors are used to bypass the high frequency noise of the input and output of the power supply. Printed board This is an universal printed board with 15 x 25 halls. Wiring terminal This terminal is used to connect a power supply wire and load. Stud This is used as the leg of the printed board.