[Menu]>[Circuits Gallery]

PIC Circuits Gallery
Remote display

On this page, I will introduce remote display with PIC16F873. The asynchronous communication function (USART) of PIC16F873 is used for this equipment. The information which is set with the control unit is displayed on the large-sized display installed in the about 10-m left place using the cable. The size of the displaying unit has 25-cm height, 40-cm width. It is not so large size. This equipment is made to inform the people who gather to the church about the number of the hymn. So, the contents to display are limited to three kinds of fixed form letters and the 3-digit figure. Red LEDs with 5-mm diameter are used for the displaying of a letter and large-sized 7 segment LEDs are used for the digit display. It is made simple composition by considering that it is easy to see and cost performance. An LED matrix which is used recently isn't used. Also, to make it easy to see displaying letters from the distant place, a purple acrylic board is used for the displaying part.
| Circuit drawing
Console unit
| Hardware
| Circuit drawing Pattern drawing(1) Pattern drawing(2) Circuit explanation Parts explanation Making process
Software
| Flow chart List Processing explanation
Display unit
| Hardware
| Circuit drawing Pattern drawing(1) Pattern drawing(2) Circuit explanation Parts explanation Making process
Software
| Flow chart List Processing explanation
Improvement